Author: lucy.cowen

CARE POINT
Correct Documentation of Drying Operation

The date the collars are first removed from the drying rack (must be 16 hours after being machine rolled)

The first operator that removes the collars from the drying rack

If the operation is not required (hand rolled collars) - enter “N/A”. Or note if the drying has been accelerated in the hot cupboard/oven.

CARE POINT

24/02/2014