Author: lucy.cowen

CARE POINT
VERIFICATION OF ANODISATION

PURPOSE: visual aid to help assess if supplied metal has been anodised or not.
ITEM: MBEU99198 (MARTIN BAKER)
CPN000098446 (JAMES WALKER)

HOW TO USE IT:
INSPECT IN GOOD LIGHT 10% OF METALS ,PICKED RAMDOMLY FROM SUPPLIED LOT
CORRECT ANODISED PARTS APPEAR GREY AND DULL (SEE PICTURE LEFT), THOSE ARE OK TO USE
NON-ANODISED PARTS APPEAR SILVERY AND SHINY (PICTURE RIGHT), THOSE MUST BE REJECTED
VERIFY CONSIGNMENT HAS BEEN RECEIVED WITH ANODISATION C OF C AND FILE ACCORDINGLY
Communicate immediately to Buyer/ Supplier Quality if a) arrived metal is suspect/ reject or/ and
b) goods arrived without anodisation C of C

OK

OK

REJECT

REJECT

Grey and matt appearance

Silvery and shiny appearance

CARE POINT

05/05/2015